The Compact E.O.S. is composed of two integrated modules: the well known Agfa daylight system and the Agfa Classic E.O.S. film processor. The small footprint enables it to be installed even in restricted spaces. The Compact E.O.S. can be extended at the back with a table for film processing from a darkroom.
- capacity: up to 240 films per hour (medium format)
  - cassette cycle time: 15 s
  - film formats: 18 x24cm to 35 x 43cm
  - film storage magazines that can be used: Curix, Scopix
  - loading and unloading module with 7 dispensers
  - integrated time switch for automatically switching on and off at preselected times
  - stand-by circuit
  - water economy circuit for the integrated film processor
  - film surface scanning for optimum regeneration depending on the film throughput
  - infrared cold air drier offers reduced power consumption with lower heat dissipation
  - interactive operating display that shows operating state and possible service messages