The following files are firmware images that should work on most ESP32-C2-based
boards with at least 4MiB of flash and 26MHz crystal frequency. This includes
ESP8684-WROOM and ESP8684-MINI modules.

If your board has only 2MiB of flash, you should try the FLASH\_2M variant
