.. _psoc_edge_general:

.. include:: links.rst

General information about the PSOC™ Edge port
==============================================

The PSOC™ Edge is designed for next generation responsive compute and control applications, featuring hardware-assisted machine learning (ML) acceleration.
The PSOC™ Edge devices are based on high performance Arm® Cortex®-M55, including Helium™ DSP support paired with Arm® Ethos™-U55 and Cortex®-M33 paired Infineon’s ultra-low power NNLite neural network accelerator.

The PSOC™ Edge port supports boards powered by the `Infineon PSOC™ Edge family of microcontrollers <https://www.infineon.com/products/microcontroller/32-bit-psoc-arm-cortex/32-bit-psoc-edge-arm>`_ and currently supports the following MCUs:

* PSOC™ Edge E84

.. _Supported boards:

Supported boards
^^^^^^^^^^^^^^^^^

The following boards are supported on this port:

.. list-table::
   :widths: 20 20 50
   :header-rows: 1

   * - Board name
     - Connectivity
     - Special feature 
   * - KIT_PSE84_AI
     - Wi-Fi, BT
     - 60GHz radar, analog microphone, digital microphone, barometric pressure sensor, external flash, speaker interface, IMU sensor, magnetometer, image sensor
    

For more hardware-related details, refer to the following sections.

KIT_PSE84_AI
------------

Pinout
******

.. image:: img/kit_pse84_ai_pinout.png
        :width: 500

    
Technical specifications
************************
Links for product details:

* `KIT_PSE84_AI PSOC™ Edge E84 AI product page <pse84_kit_ai_product_page_>`_
* `KIT_PSE84_AI PSOC™ Edge E84 AI Kit guide <pse84_kit_ai_guide_>`_  
* `PSOC™ Edge E8x2, E8x3, E8x5, E8x6 Consumer Datasheet <pse8x_consumer_datasheet_>`_
* `PSOC™ Edge E8x2, E8x3, E8x5, E8x6 Architecture Reference Manual <pse8x_arch_ref_manual_>`_